**Specification & Firm Price Quotation in Accordance with BS 6576: 1985**

**DPC Chemical Injection**

To treat externally feature brick solid walling to the front and left side flank wall.

The system requires 112 m.m. diameter holes to be drilled at horizontal centres no

greater than 120 m.m. in depth directly into the mortar course at the base of all perpend

bedding joints.

Once the concentrated cream is installed and sealed it uses the moisture contained

In the damp wall to diffuse before curing to form a water repellent resin barrier.

The Dryzone system is backed by the Biokil Crown 30 year Underwritten Guarantee

Scheme.

Total Cost:

Only available in conjunction with Pro Clear Weather proofing

**Terms**: **One third by initial payment. Final balance due upon completion.**

To accept this firm price limited offer please sign and return this quotation retaining a file copy

Signed \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **File Copy**