# **SPECIFICATION:** To provide a **resin bonded/vapour permeable** decorative and protective specialist exterior **weather proof** wall treatment with **insulation** to all pebble dashed elevations.

**Preparation:** To include some or all of the following elements where necessary. *Biocide* cleansing of the wall surface where necessary to inhibit any further **algae contamination***.*

*Scarifying* to remove all loose and friable deposits. *Hammer Testing* of any existing cement rendered smooth/pebble or tyrolean surface to locate hollow or blown areas. *Re-rendering* with *Unibond* building adhesive. Routing of visible cracking and flat knife filling with a two pack epoxy fixative. Bagging of the entire surface to **reduce the heavy profile** with a modified, washed sand and cement slurry.

**Application:** To include *Masking* of all windows, doors and insitu fixtures & fittings. *Sheeting* with thermo plastic decking all walk ways. **Hessian** **coverage** for all adjacent shrubs and foliage.

The first application of **active resin** saturation key coat will be followed by a second pressure application of **Treatex weather proofing** at 100 PSI of not less than one kilo per square metre specifically manufactured in your choice of colour.

#### **Completion**: Site cleansing and clearance of all debris with a final inspection of completed workmanship by the Supervising Crew Operative in conjunction with the property owners whereupon the satisfaction note will be presented for approval and signature.

#### **Guarantee**: Comprehensive, independently insured cover for a period of **Twenty years** from the date of completion on all masonry type surfaces with thirty-five years proof of performance plus BBA support. **Optional independent insurance backed warranty also available**.

#### **After Sales Service**

#### Specially formulated for hand application, **five-litre colour coded** touch repair canister retained on site for minor alterations, and replaced as and when required throughout the guarantee period.