**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 001  MODEL  SERIAL | Monitor  C02030202 | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  <0.10  Y | P | MAIN OFFICE | 13 AMP |
| 002  MODEL  SERIAL | Kettle Lead | 1 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 003  MODEL  SERIAL | Kettle Lead | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.08  >19.99  N/A  Y | P | MAIN OFICE | 13 AMP |
| 004  MODEL  SERIAL | 4 Way Lead | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.02  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 005  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.11  >19.99  0.53  Y | P | MAIN OFFICE |  |
| 006  MODEL  SERIAL | HP PRINTER | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.11  >19.99  0.53  Y | P | MAIN OFFICE |  |
| 007  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | CHANGED PLUG  13 AMP |
| 008  MODEL  SERIAL | PRINTER  KYOCERA  FBC5025N | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  0.33  Y | P | MAIN OFFICE | 13 AMP |
| 009  MODEL  SERIAL | TV  GOODMANS  PT29CA0923 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE | 5 AMP |
| 010  MODEL  SERIAL | TV  GOODMANS  PT29CD1378 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE | 5 AMP |

**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 0011  MODEL  SERIAL | TV RECIEVER  0682 | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  <0.10  Y | P | MAIN OFFICE |  |
| 0012  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP  CHANGED PLUG |
| 0013  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFICE | 13 AMP  CHANGED PLUG |
| 0014  MODEL  SERIAL | HP MONITOR  CNC54915BY | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.60  Y | P | MAIN OFFICE |  |
| 0015  MODEL  SERIAL | HP COMPUTER  CZC069OFXY | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.07  >19.99  0.50  Y | P | MAIN OFFICE |  |
| 0016  MODEL  SERIAL | SPEAKERS  ALTEC  A0940BS | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 0017  MODEL  SERIAL | 4 WAY EXTENSION  LEAD | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0018  MODEL  SERIAL | 4 WAY EXTENSION  LEAD | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0019  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 020  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |

**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 0021  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0022  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP  CHANGED PLUG |
| 0023  MODEL  SERIAL | HP MONITOR  CNN5521495 | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFICE |  |
| 0024  MODEL  SERIAL | HP MONITOR  CNN55241H1 | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 0025  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | CHANGED PLUG  13 AMP |
| 0026  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.07  >19.99  0.49  Y | P | MAIN OFFICE |  |
| 0027  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  0.50  Y | P | MAIN OFFICE |  |
| 0028  MODEL  SERIAL | SPEAKER  LABTEC | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE | 3 AMP |
| 0029  MODEL  SERIAL | MIXER  DESICATE | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.09  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 030  MODEL  SERIAL | ROUTER  702134063 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |

**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 0031  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.01  >19.99  N/A  Y | P | MAIN OFFICE | 5 AMP |
| 0032  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0033  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFICE | 5AMP |
| 0034  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0035  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.07  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0036  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0037  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0038  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 0039  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |
| 040  MODEL  SERIAL | KETLLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |

**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 0041  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFFICE | 5 AMP |
| 0042  MODEL  SERIAL | 4 WAY  EXTENSION  LEAD | 2 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.01  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0043  MODEL  SERIAL | 4 WAY  EXTENSION  LEAD | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.05  >19.99  N/A  Y | P | MAIN OFICE | 13 AMP |
| 0044  MODEL  SERIAL | 4 WAY  EXTENSION  LEAD | 2 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.03  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0045  MODEL  SERIAL | 4 WAY  EXTENSION  LEAD | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  N/A  Y | P | MAIN OFFICE | 13 AMP |
| 0046  MODEL  SERIAL | HP MONITOR  55240RS | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.50  Y | P | MAIN OFFICE |  |
| 0047  MODEL  SERIAL | HP MONITOR  5511NPW | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 0048  MODEL  SERIAL | HP MONITOR  55240RZ | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.49  Y | P | MAIN OFFICE |  |
| 0049  MODEL  SERIAL | HP MONITOR  55241GJ | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.50  Y | P | MAIN OFFICE |  |
| 050  MODEL  SERIAL | KETTLE LEAD | 1 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  N/A  Y | P | MAIN OFFICE | 5AMP |

**PATLEC SERVICES - PORTABLE APPLIANCE TESTING ASSET REGISTER**

**Client: Gavin Harris**

**Reading 107 FM**

**Radio House**

**Madejski Stadium**

**Reading RG2 0FN**

**Test Date: 25 /08/12 Re-Test Date 25/08/13 Test Engineer: Colin Hyland**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Asset No:** | **Item** | **Class** | **Re**  **Test** | **Test Name** | **Reading** | **Pass**  **Fail** | **Room** | **Comment / Fuse** |
| 0051  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.07  >19.99  0.49  Y | P | MAIN OFFICE |  |
| 0052  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.06  >19.99  0.52  Y | P | MAIN OFFICE |  |
| 0053  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  0.50  Y | P | MAIN OFICE |  |
| 0054  MODEL  SERIAL | HP COMPUTER | 1 | 12 | Earth (Cont) Ohm    Insulation MOhm  Sub Leakage mA  Visual Check | 0.04  >19.99  0.49  Y | P | MAIN OFFICE |  |
| 0055  MODEL  SERIAL | SPEAKERS  CREATIVE  5BS260 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 0056  MODEL  SERIAL | SPEAKERS  LABTECH  50189B | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE | 3 AMP |
| 0057  MODEL  SERIAL | SPEAKERS  LOGITECH  5-0156B | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE |  |
| 0058  MODEL  SERIAL | HP POWER  ADAPTOR  041224.00 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.17  Y | P | MAIN OFFICE |  |
| 0059  MODEL  SERIAL | POWER SUPPLY | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.15  Y | P | MAIN OFFICE |  |
| 060  MODEL  SERIAL | LAMINATOR  LM120 | 2 | 12 | Earth (Cont) Ohm  Insulation MOhm  Sub Leakage mA  Visual Check | N/A  >19.99  0.10  Y | P | MAIN OFFICE | 3AMP |